================================================================
CRAFTEKER | Laser Calibration Card & Material Guide
================================================================

HI THERE, MAKER!
Thank you for downloading the Universal Calibration Card.
This file is designed to save you time, money, and sanity.

--- HOW TO USE THIS FILE ---
1. Import the .svg file into your laser software (LightBurn, XCS, etc.).
2. Set BLACK lines to CUT.
3. Set RED lines to ENGRAVE/SCORE.
4. Run the test on a scrap piece of your material.
5. If the 3mm slots fit perfectly -> Write down these settings!

----------------------------------------------------------------
⚠️ THE "3MM" LIE: WHY YOU NEED THIS CARD
----------------------------------------------------------------

Most plywood on the market is a gamble.
You buy "3mm" sheets, but what you actually get is 2.4mm or 2.6mm.
Your joints are loose, and your projects fall apart.

Even worse? HIDDEN GLUE POCKETS.
We know the pain of hitting a glue pocket halfway through a job. 
The laser won't cut through it, and the whole sheet is wasted.

----------------------------------------------------------------
THE SOLUTION: TRUE 3MM BASSWOOD BY CRAFTEKER
----------------------------------------------------------------

We don't play games with thickness.
Our Premium Basswood is engineered for Laser Cutters specifically.

✅ TRUE THICKNESS: We aim for 3.0mm (±0.2mm tolerance).
✅ ZERO GLUE POCKETS: Clean cuts in one pass. No uncut spots.
✅ DEAD FLAT: No warping. No pins needed.

Don't let bad wood ruin good designs.

👉 GET THE PREMIUM WOOD HERE:
>>> https://crafteker.com/shop <<<

(Limited stock available for Prime delivery)

----------------------------------------------------------------
Happy Creating!
The Crafteker Team
www.crafteker.com